**Computer Network**

**Mid Term**

**---------------------------------------------------------------------------------------------------------------------**

**Use the Layered Architecture implements the following tasks**

**Task: Sliding window control protocol with 1% frame loss at sender side and 3% frame loss at receiver side**

Implement a sliding window as a queue of size 'k' (value is specified in omnetpp.ini file) at sender and receiver’s Data-link layer.